  
Driver installation
===================
 
Run the Setup.exe, 

1/	Make sure that you install into the citect\bin directory, normally 
	"\Program Files(x86)\Schneider Electric\Citect 7.50\Bin"
2/	Install the PSDIRECT backend driver
3/	Run the driver configurator (SIXDIDW.EXE) and "Save As" the configuration file 
	to your citect project directory, this causes the driver to ask :
	"Do you wish this to be the new startup configuration ?" - Yes
	This directory is usually "\ProgramData\Schneider Electric\CitectSCADA 7.50\user\<project>
	Saving here causes the configuration to be backed up with the project






If you intend speaking to the PLC's Using ISO protocol, you need to install the ISO transport (supplied).  This is not required for TCP/IP


Installation of the ISO transport (Not required if using TCP/IP)
=================================


This driver requires a Protocol called "Siemens ISO Transport" to be loaded in the machines network settings.

You install the ISO transport and it is operational on all installed ethernet cards and operates along side any other transports already installed e.g. TCP/IP this means that you can share the H1 and office networks without any problems.


proceed with the following steps to install the ISO transport (assuming that an Ethernet card is installed and configured):

1/	open the Network and Sharing centre
2/	click the Ethernet adapter >> status page, click properties
3/	click Install
4/	select "protocol" then press Add
5/	press Have Disk
6/	enter or browse to the following path <Driver setup disk>\Win7-2012S(64bit)\
7/	press OK
8/	You will see a prompt "ISO transport for Siemens H1" if it found the correct directory
9/	press "OK"
10/	close & restart the computer



